**Method Statement: To use one shot drain cleaner**

|  |  |
| --- | --- |
| **Contract Manager:** Dave Milford | **Site Supervisor:** |
| **Originator:** G.Pinder **Position:** Health & Safety manager **Date:** 01.02.19 | |
| This method statement is critical to the health & safety of the activity(ies) it relates to. It is to be strictly adhered to. Any deviation must first be authorized by the site supervisor. | |
| **Planned Task/Activity Description:** To use One Shot Drain Cleaner | |
| **Location and Access:** (attached plan as appropriate)  Various | |
| **Working Environment & Restrictions:**  Toilets and Sink areas | |
| **Protection of others:**  Only contractors to be present during activity. | |
| **Emergency Procedures:**  Normal site emergency procedures apply. | |
| **Operatives Competence:**  Operative to be deemed to be competent | |
| **Personal Protective Equipment:**  Safety shoes.  Safety goggles.  General protective gloves. | |
| **Plant & Equipment:**  Not applicable | |
| **Materials Handling/Storage & Safety Information:**  Relevant data sheets to be followed. | |
| **Critical Stages:** (must be undertaken in correct sequence).   1. On arrival site contact made and site induction undertaken. 2. Access and check the site log book and asbestos register, collect the equipments manufacturer’s specifications (if available) and complete the site permit to work (if required). 3. Ensure there is sufficient lighting available for the procedure. 4. Follow COSHH data sheet for one shot. 5. Work area to be kept tidy at all times. 6. Clear away all equipment/materials and leave in a safe condition. 7. Report back to site contact, sign off 8. Tools and equipment will be packed away in vehicle and site cleared of materials. | |